{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Stückliste"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Stückliste","index":0,"n_rows":215,"n_cols":7,"rows_kept":215,"cut":false,"hidden":false,"merged":[[0,0,0,2]],"flags":["formulas_cached_only"]}
["Stückliste LC-80ex V2    Stand: 15.01.2016"]
[]
["Nummer","Art","Wert/Typ","Rastermaß (mm)","Koordinaten","Bemerkung","Reichelt Art.Nr."]
[]
[1,"Widerstand","10k","12,5","C1"]
[2,"Widerstand","10k","10/12,5","D1","Pullup für DCD. Nur bestücken, wenn DCD nicht extern genutzt wird."]
[3,"Widerstand","10k","10 (12,5)","A1 (B2)","Mit Batteriebackup  f. S5 oben (A1) bestücken,  ansonsten neben R4 (B2)"]
[4,"Widerstand","10k","12,5","B2"]
[5,"Widerstand","10k","12,5","B2"]
[6,"Widerstand","10k","12,5","B2"]
[7,"Widerstand","10k","12,5","B2"]
[8,"Widerstand","10k","12,5","B2"]
[9,"Widerstand","10k","12,5","B2"]
[10,"Widerstand","10k","12,5","B2"]
[11,"Widerstand","10k","12,5","B2"]
[12,"Widerstand","10k","12,5","B2"]
[13,"Widerstand","10k","12,5","B2"]
[14,"Widerstand","10k","12,5","B2"]
[15,"Widerstand","10k","12,5","B2","Pullup MEDI"]
[16,"Widerstand","1k","10","B2"]
[17,"Widerstand","3,3k","12,5","B2"]
[18,"Widerstand","220","12,5","B2"]
[19,"Widerstand","3,3k","12,5","B2"]
[20,"Widerstand","220","12,5","B2"]
[21,"Widerstand","3,3k","12,5","B2"]
[22,"Widerstand","220","12,5","B2"]
[23,"Widerstand","3,3k","12,5","B2"]
[24,"Widerstand","220","12,5","B2"]
[25,"Widerstand","3,3k","12,5","B2"]
[26,"Widerstand","220","12,5","B2"]
[27,"Widerstand","3,3k","12,5","B2"]
[28,"Widerstand","220","12,5","B2"]
[29,"Widerstand","3,3k","12,5","B2"]
[30,"Widerstand","220","12,5","B2"]
[31,"Widerstand","3,3k","12,5","B3"]
[32,"Widerstand","220","12,5","B3"]
[33,"Widerstand","3,3k","12,5","B2"]
[34,"Widerstand","(560)","12,5","B2","Pullup CLK-Leitung, Wert abhängig vom Typ CG1, evtl. nicht notwendig"]
[35,"Widerstand","10k","12,5","B2"]
[36,"Widerstand","10k","12,5","B2"]
[37,"Widerstand","(1,5k)","12,5","B3","am Quarzoszillator, Wert abhängig vom Typ CG1"]
[38,"Widerstand","(1,5k)","12,5","B3","am Quarzoszillator, Wert abhängig vom Typ CG1"]
[39,"Widerstand","10k","10","A3","Pullup INT"]
[40,"Widerstand","330","12,5","B/C3"]
[41,"Widerstand","10k","10","D3"]
[42,"Widerstand","100k","10","D3"]
[43,"Widerstand","10k","10","D3"]
[44,"Widerstand","10k","10","D3"]
[45,"Widerstand","100k","10","D3"]
[46,"Widerstand","47k","10","D3"]
[47,"Widerstand","10k","10","D3"]
[48,"Widerstand","10k","10","D3"]
[49,"Widerstand","10k","10","D3"]
[50,"Widerstand","330","10","D3"]
[51,"Widerstand","470","10","D3"]
[52,"Widerstand","10k","10","D3"]
[53,"Widerstand","10k","10","D3"]
[54,"Widerstand","1k","10","D3"]
[55,"Widerstand","10k","12,5","A4"]
[56,"Widerstand","10k","12,5","A4"]
[57,"Widerstand","10k","12,5","A4"]
[58,"Widerstand","10k","12,5","A4"]
[59,"Widerstand","10k","12,5","A4"]
[60,"Widerstand","10k","12,5","A4"]
[61,"Widerstand","10k","12,5","C4"]
[62,"Widerstand","10k","12,5","C4"]
[63,"Widerstand","10k","12,5","C4"]
[64,"Widerstand","10k","12,5","C4"]
[65,"Widerstand","10k","12,5","C4"]
[66,"Widerstand","10k","12,5","C4"]
[67,"Widerstand","10k","12,5","B2"]
[]
[1,"KerKo","100n","2,5/5","A1"]
[2,"KerKo","100n","2,5/5","A1"]
[3,"KerKo","100n","2,5/5","A1"]
[4,"KerKo","100n","2,5/5","A1"]
[5,"KerKo","100n","5","B1"]
[6,"KerKo","100n","5","B1"]
[7,"KerKo","100n","5","B1"]
[8,"Elko","100µ","2,5/5","B1"]
[9,"KerKo","100n","2,5","C1"]
[10,"KerKo","100n","2,5","C1"]
[11,"Elko","(1µ)","2,5","D1","Wert abhängig vom Typ des MAX232"]
[12,"Elko","(1µ)","2,5","D1","Wert abhängig vom Typ des MAX232"]
[13,"Elko","(1µ)","2,5","D1","Wert abhängig vom Typ des MAX232"]
[14,"Elko","(1µ)","2,5","D1","Wert abhängig vom Typ des MAX232"]
[15,"Elko","100µ","2,5","D1"]
[16,"KerKo","100n","2,5/5","D1"]
[17,"KerKo","100n","5","C1"]
[18,"KerKo","100n","2,5/5","A1"]
[19,"KerKo","100n","2,5/5","A1"]
[20,"KerKo","100n","2,5/5","B2"]
[21,"KerKo","100n","2,5/5","A2"]
[22,"KerKo","100n","2,5/5","A2"]
[23,"KerKo","100n","2,5/5","A2"]
[24,"KerKo","100n","2,5/5","A2"]
[25,"KerKo","100n","2,5/5","D2"]
[26,"KerKo","100n","2,5/5","D2"]
[27,"Elko","100µ","2,5/5","A2"]
[28,"KerKo","100n","2,5","B2"]
[29,"KerKo","100n","2,5","B2"]
[30,"KerKo","100n","2,5","C3"]
[31,"KerKo","100n","2,5/5","C2"]
[32,"Elko","1000µ (16V)","5/7,5","D2"]
[33,"Elko","1000µ (16V)","5/7,5","D2"]
[34,"KerKo","100n","2,5","B2"]
[35,"Elko","100µ","2,5/5","A3"]
[36,"Elko","1µ","2,5","B3"]
[37,"Elko","10µ","2,5","B3"]
[38,"KerKo","100n","2,5/5","D3"]
[39,"KerKo","100n","2,5/5","C3"]
[40,"KerKo","1n","5/7,5/10","D3","alternativ Folienkondensator"]
[41,"KerKo","22n","2,5/5/10","D3","alternativ Folienkondensator"]
[42,"KerKo","10n","2,5/5/10","D3","alternativ Folienkondensator"]
[43,"Elko","100µ","2,5/5","D3"]
[44,"KerKo","100n","2,5/5/7,5/10/12,5","D3","alternativ Folienkondensator, Wert vom Typ des Lautsprechers abhängig"]
[45,"KerKo","10n","2,5/5/7,5/10/15","D3","alternativ Folienkondensator"]
[46,"KerKo","100n","2,5","C3"]
[47,"KerKo","100n","2,5/5","D3"]
[]
[1,"PNP-Transistor","SF116 / 2N2904","2,5","A2","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[2,"PNP-Transistor","SF116 / 2N2904","2,5","A2","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[3,"PNP-Transistor","SF116 / 2N2904","2,5","A2","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[4,"PNP-Transistor","SF116 / 2N2904","2,5","A2","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[5,"PNP-Transistor","SF116 / 2N2904","2,5","A3","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[6,"PNP-Transistor","SF116 / 2N2904","2,5","A3","PNP-Transistor mit min. 0,5A / 600mW","2N 2904"]
[7,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[8,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[9,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[10,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[11,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[12,"PNP-Transistor","SC308 / 2N3906","2,5","B2","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[13,"PNP-Transistor","SC308 / 2N3906","2,5","B3","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[14,"PNP-Transistor","SC308 / 2N3906","2,5","B3","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[15,"PNP-Transistor","SC308 / 2N3906","2,5","C3","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[16,"PNP-Transistor","SC308 / 2N3906","2,5","D3","PNP-Transistor mit min. 0,1A / 250mW","2N 3906"]
[]
["D1","Diode","BAT86 / BAT48","7,5","A1","100 mA Schottky-Diode mit möglichst geringer Flußspannung, siehe Doku","BAT 86"]
["D2","Diode","BAT86 / BAT48","7,5","B1","100 mA Schottky-Diode mit möglichst geringer Flußspannung, siehe Doku","BAT 86"]
[]
["LED1","LED","VQA13","2,5","C3","5 mm LED rot"]
["LED2","LED","VQA23","2,5","C3","5 mm LED grün"]
[]
["CPU","Prozessor","U880 / Z80 CPU","2,5 /2,54","C1"]
["SYSTEM PIO","Z80 Peripherie","U855 / Z80 PIO","2,5 /2,54","A2","System-PIO"]
["USER PIO","Z80 Peripherie","U855 / Z80 PIO","2,5 /2,54","C3/4","User-PIO"]
["CTC","Z80 Peripherie","U857 / Z80 CTC","2,5 /2,54","C3/4"]
["SIO","Z80 Peripherie","U856 / Z80 SIO/0","2,5 /2,54","D1","Pinout paßt nur für U856 und Z80 SIO/0 !!"]
[]
["RAM1/L","RAM","U214 / U224 / 2114","2,5 /2,54","A1"]
["RAM1/H","RAM","U214 / U224 / 2114","2,5 /2,54","A1"]
["RAM2/L","RAM","U214 / U224 / 2114","2,5 /2,54","A1"]
["RAM2/H","RAM","U214 / U224 / 2114","2,5 /2,54","A1"]
["RAM3/L","RAM","U214 / U224 / 2114","2,5 /2,54","A2"]
["RAM3/H","RAM","U214 / U224 / 2114","2,5 /2,54","A2"]
["RAM4/L","RAM","U214 / U224 / 2114","2,5 /2,54","A2"]
["RAM4/H","RAM","U214 / U224 / 2114","2,5 /2,54","A2"]
[]
["ROM S1","ROM","2716 / 2732 / 2764","2,5 /2,54","C1","Weitere Typen siehe Doku (z.B. EEPROM 28C64), 2716 nur auf diesem Sockel! "]
["ROM S2","ROM","2732 / 2764","2,5 /2,54","B1","Weitere Typen siehe Doku (z.B. EEPROM 28C64)"]
["RAM/ROM S3","RAM / ROM","2732 / 2764 / 6264","2,5 /2,54","B1","wahlweise RAM oder ROM, siehe Doku"]
["RAM/ROM S4","RAM / ROM","2732 / 2764 / 6264","2,5 /2,54","B1","wahlweise RAM oder ROM, siehe Doku"]
["RAM/ROM S5","RAM / ROM","2732 / 2764 / 6264","2,5 /2,54","B1","wahlweise RAM oder ROM, siehe Doku"]
[]
["OPV1","2-fach OPV","AD822 / LT1078 / LM358","2,54","D3","Dual-OPV mit Single Supply, möglichst Rail2Rail","AD 822 AN"]
[]
["DISPLAY1","7-Segment-Anzeige","VQE23 / Toshiba TLG324","2,54","C3","2-stellige 7-Segmentanzeige mit gemeinsamer Kathode, andere Typen siehe Doku"]
["DISPLAY2","7-Segment-Anzeige","VQE23 / Toshiba TLG324","2,54","C3","2-stellige 7-Segmentanzeige mit gemeinsamer Kathode, andere Typen siehe Doku"]
["DISPLAY3","7-Segment-Anzeige","VQE23 / Toshiba TLG324","2,54","C4","2-stellige 7-Segmentanzeige mit gemeinsamer Kathode, andere Typen siehe Doku"]
[]
["VR1","Festspannungsregler","7805","2,54","D2","Festspannungsregler 5V / 1A, Pinout IN-GND-OUT"]
[]
["Z1","Schutzdiode","P6KE6V8A ","12,5","D2","Überspannungsschutzdiode 6,8V","P6KE 6,8A"]
[]
["GR1","Gleichrichter","KBU4D","5","D2","Inline Graetz-Gleichrichter >= 2A, Pinout +~~- , Pin Durchmesser max. 1,5mm","FBU4D"]
[]
["F1","Sicherungshalter","Sicherungshalter 5x20","22,5","D3",null,"PL 112000"]
[]
["L1","Entstördrossel","10-22 µH","5","D2","stehende Ausführung, Durchmesser max. 13 mm","L-07HCP 22µ"]
["L2","Entstördrossel","10-22 µH","5","D2","stehende Ausführung, Durchmesser max. 13 mm","L-07HCP 22µ"]
[]
["PW1","RS232 Pegelwandler","MAX232","2,54","D1","genauer Typ bestimmt Werte von C11 bis C14"]
[]
["AD1","3 zu 8 Decoder","DS8205 / LS138","2,5 /2,54","B2",null,"LS 138"]
["AD2","4-fach NAND Gatter","DL000 / LS00","2,5 /2,54","B2",null,"LS 00"]
["AD3","3 zu 8 Decoder","DS8205 / LS138","2,5 /2,54","B2",null,"LS 138"]
["AD4","3 zu 8 Decoder","DS8205 / LS138","2,5 /2,54","C2",null,"LS 138"]
[]
["CG1","6-fach Inverter","LS04 / DL004","2,5 /2,54","B2","Achtung, Schmitt-Trigger-Inverter (LS14) sind NICHT geeignet!","LS 04"]
["CG2","2-fach D-Flipflop","74LS74 / 7474 / D174","2,5 /2,54","C2",null,"LS 74"]
[]
["Q1","Quarz","3,6864 MHz","4,9","B2","andere Werte möglich, hängt u.a. von Software ab, siehe Doku","3,6864-HC49U-S"]
[]
["BU1","Buchse","D-Sub-Buchse 9-p. female","9,4 (7,2)","D1","Beschaltung DCE (weibliche Buchse), sowohl EU (9,4) als auch US (7,2) paßt","D-SUB BU 09EU"]
["BU2","Buchse","Hohlstecker-Buchse 5.5/2.1",null,"D3",null,"HEBW 21"]
["BU3","Buchse","DIN-Buchse 5-polig",null,"D3",null,"MABPM 5S"]
[]
["CR2032","Knopfzellenhalter","CR2032 stehend",null,"A1","nur für Batteriebackup notwendig, siehe Doku","KZH 20PCB-V"]
[]
["ohne","Profilkühlkörper","PR134/37,5/SE/M3","Maße 54x37,5 mm","D2","Platine ist für diesen Typ designt. Montage des 7805 kopfüber unten am Kühler","V 5224C"]
[]
["SPEAKER","Lautsprecher","HS77 oder Kleinlautsprecher",null,"D4","Hörkapsel, Kleinlautsprecher (>= 8 Ohm) oder Piezo, siehe Doku"]
[]
["ohne","Stiftleiste","gerade , einreihig","2,54",null,"Stiftleiste (\"Meterware\") für Jumper u.a.","MPE 087-1-050"]
[]
["ohne","Buchsenleiste","gerade , einreihig","2,54",null,"Präzisionsbuchsenleiste (\"Meterware\") als Sockel für VQE23","BL 1X20G7 2,54"]
[]
["ohne","Stiftleiste/Wannenstecker","2x25 pol. abgewinkelt","2,54","A/B4","Herausführung CPU-Bus, alternativ Platinensteckverbinder","WSL 50W"]
[]
["ohne","Stiftleiste/Wannenstecker","2x13 pol. abgewinkelt","2,54","C4","Herausführung User-Bus, alternativ Platinensteckverbinder","WSL 26W"]
[]
["ohne","Schottky-Diode","diverse je nach Ausführung",null,null,"für Diodensteckbrücken am Adressdecoder (10er Pack ordern), siehe Doku"]
[]
["ohne","Kurzhubtaster","RAFI Racon 8","7,6 x 4,5",null,"25 Stück für Tastatur","RAFI 100.503"]
["ohne","Stößel f. Kurzhubtaster","RAFI 5,5 x 7,5",null,null,"25 Stück, evtl. andere Länge, siehe Bauanleitung Tastatur","RAFI 167.091"]